# Filezilla 3 beta 11 failing to consistently resume where FZ 2 invariably works
#  First a failure when simply trying to restart the queue entry on the client
# then a Download with a successful resumable case and then a failing Download case...

Trace:	ControlSocket.cpp(948): CRealControlSocket::ContinueConnect(0022DFA0) m_pEngine=011D5C80   caller=0123CEB0
Status:	Connecting to 192.168.1.10:21...
Status:	Connection established, waiting for welcome message...
Trace:	CFtpControlSocket::OnReceive()
Response:	220-FileZilla Server version 0.9.23 beta
Trace:	CFtpControlSocket::OnReceive()
Response:	220-written by Tim Kosse (Tim.Kosse@gmx.de)
Trace:	CFtpControlSocket::OnReceive()
Response:	220 Milton Avenue
Command:	USER addmine
Trace:	CFtpControlSocket::OnReceive()
Response:	331 Password required for addmine
Command:	PASS ***********
Trace:	CFtpControlSocket::OnReceive()
Response:	230 Logged on
Status:	Connected
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Command:	CWD /HumaxMediaControllerV1.04/parts/
Trace:	CFtpControlSocket::OnReceive()
Response:	250 CWD successful. "/HumaxMediaControllerV1.04/parts" is current directory.
Command:	PWD
Trace:	CFtpControlSocket::OnReceive()
Response:	257 "/HumaxMediaControllerV1.04/parts" is current directory.
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 1
Command:	TYPE I
Trace:	CFtpControlSocket::OnReceive()
Response:	200 Type set to I
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 1
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,56)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,57)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,58)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,59)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,60)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,61)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)

##### simply stopped at this point

### Another case; here it works starting from Download operation and appends as set by default in settings...
Trace:	ControlSocket.cpp(948): CRealControlSocket::ContinueConnect(0022DFA0) m_pEngine=011D5C80   caller=0121BB20
Status:	Connecting to 192.168.1.10:21...
Status:	Connection established, waiting for welcome message...
Trace:	CFtpControlSocket::OnReceive()
Response:	220-FileZilla Server version 0.9.23 beta
Trace:	CFtpControlSocket::OnReceive()
Response:	220-written by Tim Kosse (Tim.Kosse@gmx.de)
Trace:	CFtpControlSocket::OnReceive()
Response:	220 Milton Avenue
Command:	USER addmine
Trace:	CFtpControlSocket::OnReceive()
Response:	331 Password required for addmine
Command:	PASS ***********
Trace:	CFtpControlSocket::OnReceive()
Response:	230 Logged on
Status:	Connected
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].59
Trace:	CFtpControlSocket::SendNextCommand(0)
Command:	CWD /HumaxMediaControllerV1.04/parts/
Trace:	CFtpControlSocket::OnReceive()
Response:	250 CWD successful. "/HumaxMediaControllerV1.04/parts" is current directory.
Command:	PWD
Trace:	CFtpControlSocket::OnReceive()
Response:	257 "/HumaxMediaControllerV1.04/parts" is current directory.
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 1
Command:	TYPE I
Trace:	CFtpControlSocket::OnReceive()
Response:	200 Type set to I
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 1
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,78)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 4896608
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 4896608
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].59
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 4896608
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
#~~~~~~~~~~~~~~~~~~~~~~ to save U  time, HERE is the point where the working case diverges from the fails ~~~~~~
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
:
:   < cut repeated message out here >
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CTransferSocket::OnReceive(), m_transferMode=2
Trace:	CFtpControlSocket::ResetOperation(10)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(10)
Trace:	CFtpControlSocket::ResetOperation(10)
Trace:	CControlSocket::ResetOperation(10)
Error:	Transfer aborted by user
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	Skipping reply after cancelled operation.
#                                                                                 a bit of a pause here about a minute
Status:	Disconnected from server
Trace:	CFtpControlSocket::ResetOperation(66)
Trace:	CControlSocket::ResetOperation(66)

#   That was a manual termination of the Q processing as the resume was working.
#
#  Now, this 3rd case is one that does NOT work. This ends with an Error:	Disconnected from server and dies quickly at that point

Trace:	ControlSocket.cpp(948): CRealControlSocket::ContinueConnect(0022DFA0) m_pEngine=011D5C80   caller=0121BB20
Status:	Connecting to 192.168.1.10:21...
Status:	Connection established, waiting for welcome message...
Trace:	CFtpControlSocket::OnReceive()
Response:	220-FileZilla Server version 0.9.23 beta
Trace:	CFtpControlSocket::OnReceive()
Response:	220-written by Tim Kosse (Tim.Kosse@gmx.de)
Response:	220 Milton Avenue
Command:	USER addmine
Trace:	CFtpControlSocket::OnReceive()
Response:	331 Password required for addmine
Command:	PASS ***********
Trace:	CFtpControlSocket::OnReceive()
Response:	230 Logged on
Status:	Connected
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Command:	CWD /HumaxMediaControllerV1.04/parts/
Trace:	CFtpControlSocket::OnReceive()
Response:	250 CWD successful. "/HumaxMediaControllerV1.04/parts" is current directory.
Command:	PWD
Trace:	CFtpControlSocket::OnReceive()
Response:	257 "/HumaxMediaControllerV1.04/parts" is current directory.
Trace:	CFtpControlSocket::ResetOperation(0)
Trace:	CControlSocket::ResetOperation(0)
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 1
Command:	TYPE I
Trace:	CFtpControlSocket::OnReceive()
Response:	200 Type set to I
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 1
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,79)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,80)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,81)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,82)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,83)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::FileTransfer()
Status:	Starting download of /HumaxMediaControllerV1.04/parts/20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	FileTransferSend()
Trace:	FileTransferTestResumeCapability()
Trace:	CFtpControlSocket::SendNextCommand(0)
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 2
Command:	PASV
Trace:	CFtpControlSocket::OnReceive()
Response:	227 Entering Passive Mode (192,168,1,10,4,84)
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 2
Trace:	  state = 2
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 3
Command:	REST 28487008
Trace:	CFtpControlSocket::OnReceive()
Response:	350 Rest supported. Restarting at 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 3
Trace:	  state = 3
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 4
Command:	RETR 20070722 1344 i7T4_ T4 on the Bea.ts.[76].52
Trace:	CTransferSocket::OnConnect
Trace:	CFtpControlSocket::OnReceive()
Response:	150 Connection accepted, restarting at offset 28487008
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 1
Trace:	  state = 4
Trace:	CFtpControlSocket::TransferSend(0)
Trace:	  state = 5
Trace:	CTransferSocket::OnClose
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CFtpControlSocket::TransferEnd()
Trace:	CFtpControlSocket::OnReceive()
Response:	426 Connection closed; transfer aborted.
Trace:	CFtpControlSocket::TransferParseResponse()
Trace:	  code = 4
Trace:	  state = 7
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CTransferSocket::TransferEnd(1)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::SendNextCommand(2)
Trace:	FileTransferSend()
Trace:	CFtpControlSocket::ResetOperation(2)
Trace:	CControlSocket::ResetOperation(2)
Trace:	CFtpControlSocket::OnReceive()
Response:	421 Connection timed out.
Trace:	Unexpected reply, no reply was pending.
Trace:	CRealControlSocket::OnClose()
Error:	Disconnected from server
Trace:	CFtpControlSocket::ResetOperation(66)
Trace:	CControlSocket::ResetOperation(66)
Status:	Disconnected from server
Trace:	CFtpControlSocket::ResetOperation(66)
Trace:	CControlSocket::ResetOperation(66)